**PART M66**

**AMENITY MAINTENANCE**

**CONTENTS**

1. General
2. Response Times
3. Records and Reporting
4. Additional Requirements

Maintenance Activities

RA/RP Road User Amenity Maintenance

RL/RC Litter Collection

**1. GENERAL**

This Part specifies the requirements for litter collection and road side facilities.

**2. RESPONSE TIMES**

Rectification of roadside amenity facilities (RA) shall be undertaken in conjunction with Clause M06.3.2 "Loop Inspections".

Response time for litter collection (RL) shall be undertaken in conjunction with Clause M06.3.2 "Loop Inspections".

Rectification of any specific maintenance defects (RP and RC) shall be undertaken within the timeframes agreed to between the Superintendent and the Contractor.

**3. RECORDS AND REPORTING**

The Contractor shall report on abandoned vehicles and Council registered dead animals in accordance with Clause M06.4 "Recording and Reporting Requirements".

**4. ADDITIONAL REQUIREMENTS**

**4.1. Waste Disposal**

The Contractor shall dispose of waste materials in accordance with Clause M55.9 "Waste Management".

**4.2** **Water Tanks**

The Contractor shall ensure that any water tanks are inspected for damage or leaks and filled with potable water on an as required basis.

**4.3 Litter**

Litter visible from the travelled way and within the Maintenance Activity Zone (MAZ) shall be removed at frequency specified within the intervention level. Litter visible as a result of mowing shall be removed either prior to or within 24 hours after mowing.

To remove any abandoned vehicles, the Contractor shall notify the following:

1. the Traffic Management Centre (TMC) for freeways and expressways;
2. SAPOL for road carriageways; or
3. relevant Local Council, within other maintenance activity zones

\_\_\_\_\_\_\_\_\_\_\_\_

**MAINTENANCE ACTIVITIES**

**ROAD USER AMENITY MAINTENANCE (RA/RP)**

**Application:** This standard applies to roadside facilities listed in the Appendix 19.

|  |  |  |  |
| --- | --- | --- | --- |
| **Defects** | **Intervention Level** | **Compulsory Intervention Level** | **Performance Requirement** |
| **Routine Maintenance:**  Defacing or damage to tables, toilets, litter bins, sun shelters, monuments, windsocks and water tanks (including the tap) that are repairable.  **Specific Maintenance:**  Damaged asset elements that are beyond repair. | Defects where:   * Defacing or damage to tables, litter bins, sun shelters, toilets and monuments. * Wind socks are missing, damaged or faulty. * Water tanks are empty or damaged~~.~~ * Facilities that are in an unsafe condition.   **MDR Recording:**  Defects shall be recorded on the MDR as RA.  Specific Maintenance shall be recorded on the MDR as RP. | Not applicable | **Furniture:** Tables, litter bins, sun shelters, monuments, windsocks, toilets and water tanks are functional and do not present a hazard to road users.  **Water tanks:** full of potable water, taps functional and lids secure.  **Windsocks:** Operational.  **Litter:** Litter bin lids in place and secured with locks.  **Environmental:** No vegetation within 500 mm of tables, litter bins, sun shelters, monuments, windsocks, and water tanks (including the tap). |

**MAINTENANCE ACTIVITIES**

**LITTER COLLECTION (RL/RC)**

**Application:** This standard applies to the collection and removal of roadside litter.

|  |  |  |  |
| --- | --- | --- | --- |
| **Defects** | **Intervention Level** | **Compulsory Intervention Level** | **Performance Requirement** |
| **Routine Maintenance:**  Litter or debris on the carriageway, drains, medians, at roadside rest areas, stack sites and weigh stations.  Road kill, (dead animals) on the carriageway.  Litter in bins.  Abandoned vehicles on the carriageway or in rest areas.  **Specific Maintenance:**  Car bodies removed from controlled access roads.  Hard waste comprising of general household or commercial type waste not considered as normal road user litter, including tyres greater than 5 in number from any one site. | Defects where:  Litter or debris on carriageway, in bins, roadside rest areas, stack sites and weigh stations.  Abandoned vehicles on the carriageway or in rest areas.  **MDR Recording:**  Defects shall be recorded on the MDR as RL  Specific Maintenance shall be recorded on the MDR as RC. | Defects where:   * litter or debris constitutes a hazard to road users,   Animal carcasses on the carriageway.   * Litterbins are full or ineffective, * Road users complain about litter. | **Safety:** Dead animals removed from the carriageway.  **Appearance:** No litter visible:   * from the carriageway; * within the road side rest area   **Waste management:**  Litter bins empty and lined with a plastic bag.  Litter disposed of at a licensed waste depot.  Abandoned vehicles removed from the carriageway. |